


* Help info about arp command




* Display ARP-table






* Pick network interface




* Clean ARP-table





* Check ARP-table is empty, haha not  
  
* Ping computer in local network  
  
* Stop capturing packets (Wireshark)




* Filtered ICMP and ARP only







* ARP dialog sketch
* ARP-table  
  
* 